134

| DRIVER'S DOOR WIRING
X84

#### 134
ELECTRIC REAR-VIEW MIRROR CONTROL
DD/CPE

1 | 0.35 | 40X | REAR-VIEW MIRROR FOLD OUT CONTROL
2 | 0.35 | LPG | PROTECTED LEFT HAND SIDE LIGHT +
3 | 0.35 | 40E | REAR VIEW MIRROR MOTOR COMMON
4 | 0.35 | MAN | DASHBOARD RIGHT-HAND CROSS MEMBER ELECTRICAL EARTH
5 | 0.5 | BCP3 | PROTECTED + BATTERY FEED CIRCUIT BREAKER INTERIOR LIGHT FUSE
6 | 0.35 | 40C | DRIVER'S REAR VIEW MIRROR UP/DOWN CONTROL
7 | 0.35 | 40B | PASSENGER REAR VIEW MIRROR UP/DOWN CONTROL
8 | 0.35 | 40A | DRIVER'S REAR VIEW MIRROR RIGHT>LEFT CONTROL
9 | 0.35 | 40D | PASSENGER REAR VIEW MIRROR RIGHT>LEFT CONTROL
10 | 0.35 | 40W | REAR-VIEW MIRROR FOLD IN CONTROL