R2

| CONNECTION
ANY TYPE

#### R2
DASHBOARD/LEFT REAR CONNECTION
X84 B84,S84/DG/SPRGAZ/EPACK X84 B84,S84/DG/EQGPL/EPACK

1 | 3.0 | BP87 | REAR ELECTRIC WINDOWS FUSE PROTECTED + BATTERY FEED
7 | 0.35 | BPT2 | + BATTERY PROTECTED TIMED LIGHTING
8 | 0.35 | 13AC | FOOTWELL LIGHTING TIMER + CONTROL
11 | 0.35 | 20AL | REAR INTERIOR LOCKING CONTROL
12 | 0.35 | 21K | ANTI-PINCH SUNROOF/ELECTRIC WINDOW SERIAL LINE SIGNAL
13 | 0.35 | 23A | ELECTRIC WINDOW CONTROL > RIGHT-HAND REAR QUARTER LIGHT CLOSE
14 | 0.35 | 23B | ELECTRIC WINDOW DOWN CONTROL > RIGHT HAND REAR QUARTER LIGHT OPEN
15 | 0.35 | 23C | ELECTRIC WINDOW UP CONTROL > LEFT HAND REAR QUARTER LIGHT CLOSE
16 | 0.35 | 23D | ELECTRIC WINDOW DOWN CONTROL > LEFT HAND REAR QUARTER LIGHT OPEN
17 | 0.35 | 23G | RIGHT HAND REAR ELECTRIC WINDOW CONTROL 1
18 | 0.35 | 23H | RIGHT HAND REAR ELECTRIC WINDOW CONTROL 2
19 | 0.35 | 23J | LEFT HAND REAR ELECTRIC WINDOW CONTROL 1
20 | 0.35 | 23K | LEFT HAND REAR ELECTRIC WINDOW CONTROL 2
26 | 0.35 | 26AQ | KEYLESS VEHICLE LOCKING SIGNAL / PASSENGER SIDE DOORS SWITCH
27 | 0.35 | 26AP | KEYLESS VEHICLE LOCKING SIGNAL / DRIVER SIDE DOORS SWITCH
28 | 0.5 | 26AR | KEYLESS VEHICLE LEVEL 2 LOCKING SIGNAL / BOOT LID SWITCH
29 | 0.5 | 26P | DOOR HANDLE INFRARED SENSOR +
29 | 0.5 | 26P | DOOR HANDLE INFRARED SENSOR +
30 | 0.35 | 26Q | PASSENGER SIDE DOOR HANDLE INFRARED SENSOR SIGNAL
31 | 0.35 | 26S | DRIVER'S SIDE REAR HANDLE INFRARED SENSOR SIGNAL
32 | 0.35 | 26AW | KEYLESS VEHICLE INTERIOR AERIAL 2 SIGNAL 2
33 | 0.35 | 26AV | KEYLESS VEHICLE INTERIOR AERIAL 2 SIGNAL 1
47 | 0.35 | 26AN | KEYLESS VEHICLE BOOT LID EXTERNAL AERIAL SIGNAL2
48 | 0.35 | 26AM | KEYLESS VEHICLE BOOT LID EXTERNAL AERIAL A SIGNAL
49 | 0.35 | 26AL | KEYLESS VEHICLE REAR PASSENGER DOOR EXTERNAL AERIAL B SIGNAL
50 | 0.35 | 26AK | KEYLESS VEHICLE REAR PASSENGER DOOR EXTERNAL AERIAL A SIGNAL
51 | 0.35 | 26AG | KEYLESS VEHICLE DRIVER'S SIDE REAR DOOR EXTERNAL AERIAL A SIGNAL
52 | 0.35 | 26AH | KEYLESS VEHICLE DRIVER'S SIDE REAR DOOR EXTERNAL AERIAL B SIGNAL