120

| ENGINE WIRING
F9Q814

#### 120
INJECTION COMPUTER
ANY TYPE

A1 | 0.5 | 3FJ | INJECTION COMPUTER SENSOR -
B1 | 0.75 | 3BG | ENGINE SPEED SIGNAL > TDC SENSOR
C1 | 0.75 | 3BL | ENGINE SPEED > TDC SENSOR - SIGNAL
D1 | 0.5 | 3CQ | CAMSHAFT SENSOR SIGNAL
E1 | 0.5 | 3AA | INJECTION LOCKING RELAY COIL - CONTROL
F1 | 0.75 | 38X | REFRIGERANT GAS PRESSURE SENSOR SIGNAL
G1 | 0.5 | 3DV | AIRFLOW SENSOR + SIGNAL
H1 | 0.5 | 3JK | COOLANT TEMPERATURE -
B2 | 0.5 | 3VM | AIR INTAKE FLAP FAULT FINDING
C2 | 0.75 | 3VP | CONTROL + GAS RECIRCULATION MOTOR
D2 | 0.75 | 3VQ | CONTROL - GAS RECIRCULATION MOTOR
E2 | 0.5 | 3DW | AIRFLOW SENSOR - SIGNAL
F2 | 0.5 | 3C | COOLANT TEMPERATURE SENSOR + SIGNAL
G2 | 0.5 | 3B | AIR TEMPERATURE SENSOR + SIGNAL
J2 | 0.5 | 3EL | EGR POTENTIOMETER + SIGNAL
K2 | 0.5 | 3LP | TURBOCHARGER PRESSURE SENSOR + SIGNAL
M2 | 2.0 | 3FB | INJECTION + > PROTECTIVE RELAY
F3 | 0.75 | 38Y | REFRIGERANT GAS PRESSURE SENSOR +
G3 | 0.5 | 3LY | RAIL FUEL PRESSURE SENSOR + SIGNAL
J3 | 0.75 | 47Q | OIL TEMPERATURE SENSOR + SIGNAL
A4 | 0.5 | 3LX | RAIL FUEL PRESSURE SENSOR +
B4 | 0.75 | 3KJ | AIRFLOW +
C4 | 0.5 | 3LZ | RAIL FUEL PRESSURE SENSOR -
D4 | 0.5 | 3LN | TURBOCHARGER PRESSURE SENSOR -
F4 | 0.5 | 3GC | EGR SENSOR +
G4 | 0.5 | 3LQ | TURBOCHARGER PRESSURE SENSOR +
H4 | 0.5 | 3VG | TURBOCHARGER COOLANT PUMP RELAY CONTROL
J4 | 0.5 | 3VN | CONTROL - AIR INTAKE FLAP
L4 | 1.0 | 3DU | AIRFLOW SENSOR -
M4 | 1.4 | 3HI | FUEL PRESSURE CONTROL SOLENOID VALVE - CONTROL