120

| DASHBOARD WIRING
DG

#### 120
INJECTION COMPUTER
EBASE/ABLAV EBASE/SABLAT CA,CAREG/SSESP CA,CAREG/ASRESP

D1 | 0.35 | AP15 | PROTECTED + AFTER IGNITION ENGINE FUNCTIONS FUSE
G1 | 2.0 | 3FB | INJECTION + > PROTECTIVE RELAY
H1 | 2.0 | N | ELECTRONIC EARTH
A2 | 0.35 | 3FX | CRUISE CONTROL ON>OFF - CONTROL
D2 | 0.35 | 86G | CRUISE CONTROL PROGRAMMING CONTROL
F2 | 0.35 | 3LU | + LOAD POTENTIOMETER 2
G2 | 0.75 | 3LR | + LOAD POTENTIOMETER 1
H2 | 0.75 | 3LS | LOAD POTENTIOMETER 1 + SIGNAL
A3 | 0.35 | 3SN | MOTOR 2 CAN L SIGNAL
C3 | 0.35 | 3PD | SPEED LIMITER ON/OFF CONTROL
D3 | 0.35 | 86M | CRUISE CONTROL PROGRAMMING RETURN SIGNAL
F3 | 0.35 | 3LW | LOAD POTENTIOMETER 2 + SIGNAL
H3 | 0.75 | 3LT | - LOAD POTENTIOMETER 1
A4 | 0.35 | 3SM | MOTOR 2 CAN H SIGNAL
B4 | 0.35 | HK | DIAGNOSTIC SIGNAL K
C4 | 0.35 | 86D | DECLUTCH + SIGNAL
E4 | 0.35 | 5A | BRAKE PEDAL SWITCH + SIGNAL
F4 | 0.35 | 3LV | - LOAD POTENTIOMETER 2
G4 | 2.0 | N | ELECTRONIC EARTH
H4 | 2.0 | N | ELECTRONIC EARTH