120

| ENGINE WIRING
K9K722

#### 120
INJECTION COMPUTER
CA,CAREG/SANFLT CA,CAREG/FLTDIE

F1 | 0.5 | 3AA | INJECTION LOCKING RELAY COIL - CONTROL
F2 | 0.5 | 3FF | PRE-HEATER RELAY - CONTROL
G2 | 2.0 | 3FB1 | INJECTION + > PROTECTIVE RELAY
H2 | 2.0 | 3FB1 | INJECTION + > PROTECTIVE RELAY
C3 | 0.75 | 38X | REFRIGERANT GAS PRESSURE SENSOR SIGNAL
D3 | 0.5 | 3FY | PRE-HEATER RELAY DIAGNOSTIC SIGNAL
G3 | 0.75 | 38U | RHEOSTAT CURSOR
C4 | 0.75 | 38Y | REFRIGERANT GAS PRESSURE SENSOR +
B3 | 0.5 | 3WT | WATER IN DIESEL DETECTION SENSOR SIGNAL