1076

| ENGINE WIRING
F4R770,F4R771

#### 1076
MOTORISED THROTTLE BODY
BVA4/TLMEXI BVM6 BVA4/SSTLMEXI

1 | 0.5 | 3MP | MOTORISED THROTTLE POTENTIOMETER 1 SIGNAL
2 | 0.5 | 3MN | MOTORISED THROTTLE POTENTIOMETER + 5 VOLTS
3 | 1.0 | 3AJB | THROTTLE MOTOR + CONTROL
4 | 0.5 | 3MQ | MOTORISED THROTTLE POTENTIOMETER 2 SIGNAL
5 | 1.0 | 3AJC | THROTTLE MOTOR - CONTROL
6 | 0.5 | 3MO | MOTORISED THROTTLE POTENTIOMETER SENSOR -