134

| DRIVER'S DOOR WIRING
X84

#### 134
ELECTRIC REAR-VIEW MIRROR CONTROL
B84,S84/DG/EPACK

A1 | 0.35 | 40A | DRIVER'S REAR VIEW MIRROR RIGHT>LEFT CONTROL
B1 | 0.35 | 40D | PASSENGER REAR VIEW MIRROR RIGHT>LEFT CONTROL
A2 | 0.5 | BCP3 | PROTECTED + BATTERY FEED CIRCUIT BREAKER INTERIOR LIGHT FUSE
B2 | 0.35 | 40B | PASSENGER REAR VIEW MIRROR UP/DOWN CONTROL
A3 | 0.35 | 40C | DRIVER'S REAR VIEW MIRROR UP/DOWN CONTROL
B3 | 0.35 | MAM | DASHBOARD LEFT-HAND CROSS MEMBER ELECTRICAL EARTH
B4 | 0.35 | 40E | REAR VIEW MIRROR MOTOR COMMON