140

| DRIVER'S DOOR WIRING
X84

#### 140
DRIVER'S DOOR ELECTRIC LOCKING
DD/SUPCPE

A | 0.5 | 20X | FRONT DEADLOCKING MOTOR CONTROL
B | 0.5 | 20BC | DRIVER'S DOOR / FUEL FILLER FLAP UNLOCKING MOTOR CONTROL
C | 0.35 | MAN | DASHBOARD RIGHT-HAND CROSS MEMBER ELECTRICAL EARTH
D | 0.35 | 87H | DRIVER'S 1st POSITION SWITCH - SIGNAL
E | 0.5 | 20BC | DRIVER'S DOOR / FUEL FILLER FLAP UNLOCKING MOTOR CONTROL
F | 0.5 | 20BH | DRIVER'S DOOR / FUEL FILLER FLAP LOCK MOTOR CONTROL