141

| FRONT PASSENGER DOOR WIRING
X84

#### 141
CENTRAL LOCKING FOR PASSENGER DOOR
B84,S84/DD/SUPCPE

A | 0.5 | 20BK | PASSENGER DOORS / REAR DOORS LOCKING MOTOR CONTROL
B | 0.5 | 20BD | OPEN FRONT/REAR PASSENGER DOORS MOTOR CONTROL
C | 0.35 | 87G | PASSENGER'S 1st POSITION SWITCH - SIGNAL
D | 0.35 | MAM | DASHBOARD LEFT-HAND CROSS MEMBER ELECTRICAL EARTH
E | 0.5 | 20BC | DRIVER'S DOOR / FUEL FILLER FLAP UNLOCKING MOTOR CONTROL
F | 0.5 | 20X | FRONT DEADLOCKING MOTOR CONTROL