120

| ENGINE WIRING
F9Q800,F9Q808

#### 120
INJECTION COMPUTER
F9Q800/SANFLT F9Q808 F9Q800/FLTDIE

A1 | 0.5 | 3FJ | INJECTION COMPUTER SENSOR -
B1 | 0.75 | 3BG | ENGINE SPEED SIGNAL > TDC SENSOR
C1 | 0.75 | 3BL | ENGINE SPEED > TDC SENSOR - SIGNAL
D1 | 0.5 | 3CQ | CAMSHAFT SENSOR SIGNAL
E1 | 0.5 | 3AA | INJECTION LOCKING RELAY COIL - CONTROL
F1 | 0.75 | 38X | REFRIGERANT GAS PRESSURE SENSOR SIGNAL
G1 | 0.5 | 3DV | AIRFLOW SENSOR + SIGNAL
H1 | 0.5 | 3JK | COOLANT TEMPERATURE -
E2 | 0.5 | 3DW | AIRFLOW SENSOR - SIGNAL
F2 | 0.5 | 3C | COOLANT TEMPERATURE SENSOR + SIGNAL
G2 | 0.5 | 3B | AIR TEMPERATURE SENSOR + SIGNAL
H2 | 0.5 | 3FAB | FUEL TEMPERATURE + SIGNAL
J2 | 0.5 | 3EL | EGR POTENTIOMETER + SIGNAL
K2 | 0.5 | 3LP | TURBOCHARGER PRESSURE SENSOR + SIGNAL
L2 | 1.0 | 3GB | EGR SOLENOID VALVE -
M2 | 2.0 | 3FB1 | INJECTION + > PROTECTIVE RELAY
F3 | 0.75 | 38Y | REFRIGERANT GAS PRESSURE SENSOR +
G3 | 0.5 | 3LY | RAIL FUEL PRESSURE SENSOR + SIGNAL
A4 | 0.5 | 3LX | RAIL FUEL PRESSURE SENSOR +
B4 | 0.5 | 3KJ | AIRFLOW +
C4 | 0.5 | 3LZ | RAIL FUEL PRESSURE SENSOR -
D4 | 0.5 | 3LN | TURBOCHARGER PRESSURE SENSOR -
F4 | 0.5 | 3GC | EGR SENSOR +
G4 | 0.5 | 3LQ | TURBOCHARGER PRESSURE SENSOR +
J4 | 0.5 | 3KG | INLET FLAP SOLENOID VALVE - CONTROL
L4 | 1.0 | 3WV | - FLOWMETER
M4 | 1.4 | 3HI | FUEL PRESSURE CONTROL SOLENOID VALVE - CONTROL