225

| DASHBOARD WIRING
DG

#### 225
DIAGNOSTIC SOCKET
EBASE/ABLAV EBASE/SABLAT CA,CAREG/SSESP CA,CAREG/ASRESP

1 | 0.5 | AP43 | PROTECED + AFTER IGNITION FUSE
4 | 0.35 | MAN | DASHBOARD RIGHT-HAND CROSS MEMBER ELECTRICAL EARTH
5 | 0.35 | NAM | UPPER LEFT-HAND CROSS MEMBER ELECTRONIC EARTH
6 | 0.35 | 133B | INSTRUMENT PANEL CAN H SIGNAL > COMPUTER
7 | 1.0 | HK | DIAGNOSTIC SIGNAL K
14 | 0.35 | 133C | INSTRUMENT PANEL CAN L SIGNAL > COMPUTER
16 | 0.5 | BP32 | PROTECTED + BATTERY FEED HORN FUSE