240

| FRONT PASSENGER DOOR WIRING
X84

#### 240
PASSENGER ELECTRIC REAR-VIEW MIRROR
B84,S84/DG/EPACK B84,S84/DG/EPACKP

1 | 0.35 | 15RP | PROTECTED HEATED REAR VIEW MIRROR + CONTROL
2 | 0.35 | 40B | PASSENGER REAR VIEW MIRROR UP/DOWN CONTROL
3 | 0.35 | 40E | REAR VIEW MIRROR MOTOR COMMON
4 | 0.35 | 40D | PASSENGER REAR VIEW MIRROR RIGHT>LEFT CONTROL
5 | 0.35 | MAN | DASHBOARD RIGHT-HAND CROSS MEMBER ELECTRICAL EARTH
6 | 0.35 | 47C | EXTERNAL TEMPERATURE SENSOR + SIGNAL
7 | 0.35 | 40W | REAR-VIEW MIRROR FOLD IN CONTROL
9 | 0.35 | 40X | REAR-VIEW MIRROR FOLD OUT CONTROL
10 | 0.35 | 47D | EXTERNAL TEMPERATURE SENSOR ZERO VOLTS SIGNAL