1337

| FRONT END WIRING
X84

#### 1337
SWITCHING PROTECTION UNIT
SPROJA/SLDECH PROJAB/SLDECH

1 | 0.35 | LPG | PROTECTED LEFT HAND SIDE LIGHT +
2 | 0.35 | LPD | PROTECTED RIGHT HAND SIDE LIGHT +
3 | 1.0 | RPG | LEFT HAND PROTECTED MAIN BEAM HEADLIGHT +
4 | 1.0 | RPD | RIGHT HAND PROTECTED MAIN BEAM HEADLIGHT +
5 | 0.5 | CPD | PROTECTED RIGHT HAND DIPPED BEAM HEADLIGHT +
5 | 0.5 | CPD | PROTECTED RIGHT HAND DIPPED BEAM HEADLIGHT +
6 | 0.5 | CPG | PROTECTED LEFT HAND DIPPED BEAM HEADLIGHT +
6 | 0.5 | CPG | PROTECTED LEFT HAND DIPPED BEAM HEADLIGHT +
7 | 0.5 | 8F | + FRONT RIGHT-HAND FOG LIGHTS > RESISTANCE
8 | 0.5 | 8E | + FRONT LEFT-HAND FOG LIGHTS > RESISTANCE