645

| DASHBOARD WIRING
DG

#### 645
PASSENGER COMPARTMENT COMPUTER
EBASE/ABLAV EBASE/SABLAT CA,CAREG/SSESP CA,CAREG/ASRESP

1 | 0.35 | 26J | CONTROL - SAFETY HALL SENSOR
2 | 0.35 | 47Z | EXTERNAL TEMPERATURE / DISPLAY SIGNAL
3 | 0.35 | 64F | HAZARD WARNING LIGHTS INDICATOR LIGHT + CONTROL
4 | 0.35 | 26BC | CARD LOCATION ELECTROLUMINESCENT DIODE CONTROL
5 | 0.35 | 26X | CLUTCH - SIGNAL
6 | 0.35 | 20AW | ONE-TOUCH DOOR LOCKING/UNLOCKING CONTROL
7 | 0.35 | 26N | ENGINE START/STOP + SIGNAL
8 | 0.5 | 87T | BOOT LID POSITION SWITCH 1 SIGNAL
12 | 0.5 | 16A | WINDSCREEN WASHER PUMP + CONTROL
13 | 0.35 | 26M | ENGINE RUNNING WARNING LIGHT CONTROL
14 | 0.35 | 20M | DOOR LOCKING LED
15 | 0.22 | 87G | PASSENGER'S 1st POSITION SWITCH - SIGNAL
16 | 0.35 | 87B | RIGHT HAND REAR 1st POSITION SWITCH - SIGNAL
17 | 0.22 | 87H | DRIVER'S 1st POSITION SWITCH - SIGNAL
19 | 0.35 | 87A | LEFT HAND REAR 1st POSITION SWITCH - SIGNAL
9 | 0.35 | 20T | CHILD SAFETY LED - CONTROL
11 | 0.35 | 20AL | REAR INTERIOR LOCKING CONTROL
18 | 0.75 | 20BG | REAR DOORS DEADLOCKING STATUS SIGNAL