260

| DASHBOARD WIRING
DG

#### 260
PASSENGER COMPARTMENT FUSE BOX AND RELAY
EBASE/ABLAV

1B | 2.5 | BP77 | BATTERY PROTECTED + FEED > UCH
1C | 4.0 | SP16 | PROTECTED + ACCESSORIES FEED / ACCESSORIES FEED FUSE SUPPLY
1D | 4.0 | BP11 | PROTECTED + BATTERY FEED > PASSENGER COMPARTMENT 1
1E | 4.0 | BP11 | PROTECTED + BATTERY FEED > PASSENGER COMPARTMENT 1
1F | 0.5 | SP15 | PROTECTED + ACCESSORIES FEED FUSE
1F | 0.75 | SP15 | PROTECTED + ACCESSORIES FEED FUSE
1G | 3.0 | SP2 | PROTECTED + ACCESSORIES > RADIO
1H | 2.0 | SP17 | PROTECTED + ACCESSORIES FEED > BRAKE LIGHTS FUSE
1L | 1.4 | BP55 | DRIVER'S ONE-TOUCH ELECTRIC WINDOW FUSE PROTECTED + BATTERY FEED
1N | 2.5 | BCP3 | PROTECTED + BATTERY FEED CIRCUIT BREAKER INTERIOR LIGHT FUSE
1O | 3.0 | BP32 | PROTECTED + BATTERY FEED HORN FUSE
1P | 1.4 | BP25 | PROTECTED + BATTERY FEED REAR SCREEN WIPER
1R | 3.0 | BP77 | BATTERY PROTECTED + FEED > UCH
1T | 3.0 | BP11 | PROTECTED + BATTERY FEED > PASSENGER COMPARTMENT 1
1U | 3.0 | BPS1 | + BATTERY SAFETY PROTECTED
2B | 0.5 | S | + ACCESSORIES FEED
2C | 4.0 | SP3 | PROTECTED + ACCESSORIES > HEATER
2D | 3.0 | BP48 | PROTECTED + BATTERY FEED > ELECTRIC WINDOW
2E | 1.0 | BP93 | + BATTERY PROTECTED SUNROOF
2G | 5.0 | SP16 | PROTECTED + ACCESSORIES FEED / ACCESSORIES FEED FUSE SUPPLY
2L | 5.0 | BP12 | PROTECTED + BATTERY FEED > PASSENGER COMPARTMENT 2
2O | 5.0 | BP12 | PROTECTED + BATTERY FEED > PASSENGER COMPARTMENT 2
2T | 2.0 | BPR1 | + BATTERY FEED > RELAY
2U | 3.0 | BP3 | PROTECTED + BATTERY FEED ELECTRIC DOOR LOCKING
3B | 5.0 | BP12 | PROTECTED + BATTERY FEED > PASSENGER COMPARTMENT 2
5B | 5.0 | SP16 | PROTECTED + ACCESSORIES FEED / ACCESSORIES FEED FUSE SUPPLY
1A | 0.5 | AP43 | PROTECED + AFTER IGNITION FUSE
2A | 0.35 | MAM | DASHBOARD LEFT-HAND CROSS MEMBER ELECTRICAL EARTH
3A | 3.0 | BP48 | PROTECTED + BATTERY FEED > ELECTRIC WINDOW
5A | 3.0 | A1 | + AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY