645

| DASHBOARD WIRING
DD

#### 645
PASSENGER COMPARTMENT COMPUTER
ANY TYPE

1 | 0.35 | 14S | RAIN SENSOR SERIAL LINE SIGNAL
2 | 0.22 | 141H | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL LINE 5 SIGNAL
3 | 0.35 | 47C | EXTERNAL TEMPERATURE SENSOR + SIGNAL
4 | 0.22 | 141D | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL LINE 3 SIGNAL
5 | 0.22 | 141N | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL COLUMN 4 SIGNAL
6 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL
7 | 0.5 | 21K | ANTI-PINCH SUNROOF/ELECTRIC WINDOW SERIAL LINE SIGNAL
8 | 0.5 | 133B | INSTRUMENT PANEL CAN H SIGNAL > COMPUTER
9 | 0.22 | 141K | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL COLUMN 1 SIGNAL
10 | 0.35 | 26AZ | KEYLESS VEHICLE STEERING COLUMN LOCK CAN H SIGNAL
11 | 0.22 | 141G | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL LINE 4 SIGNAL
12 | 0.22 | 141C | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL LINE 2 SIGNAL
13 | 0.35 | 47D | EXTERNAL TEMPERATURE SENSOR ZERO VOLTS SIGNAL
14 | 0.22 | 141B | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL LINE 1 SIGNAL
15 | 0.22 | 141L | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL COLUMN 2 SIGNAL
16 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL
17 | 0.22 | 141M | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL COLUMN 3 SIGNAL
18 | 0.5 | 133C | INSTRUMENT PANEL CAN L SIGNAL > COMPUTER
19 | 0.22 | 141P | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL COLUMN 5 SIGNAL
20 | 0.35 | 26BA | KEYLESS VEHICLE STEERING COLUMN LOCK CAN L SIGNAL