261

| RADIO/MULTIMEDIA DISPLAY INTERMEDIATE WIRING
DD

#### 261
RADIO
RAD04

1 | 0.22 | 47F | VEHICLE SPEED SIGNAL
3 | 0.35 | 107D | TELEPHONE RADIO CUT-OFF SIGNAL
4 | 1.0 | BCP3 | PROTECTED + BATTERY FEED CIRCUIT BREAKER INTERIOR LIGHT FUSE
5 | 0.35 | 34AM | WAVE SEPARATOR AERIAL AMPLIFIER +
7 | 1.0 | SP2 | PROTECTED + ACCESSORIES > RADIO
8 | 3.0 | MAW | REAR RIGHT-HAND WHEEL ARCH RADIO ELECTRICAL EARTH
9 | 1.0 | 34D | RIGHT HAND REAR LOUDSPEAKER + SIGNAL
10 | 1.0 | 34C | RIGHT HAND REAR LOUDSPEAKER - SIGNAL
11 | 1.4 | 34E | RIGHT HAND FRONT LOUDSPEAKER + SIGNAL
12 | 1.4 | 34F | RIGHT HAND FRONT LOUDSPEAKER - SIGNAL
13 | 1.4 | 34G | LEFT HAND FRONT LOUDSPEAKER + SIGNAL
14 | 1.4 | 34H | LEFT HAND FRONT LOUDSPEAKER - SIGNAL
15 | 1.0 | 34A | LEFT HAND REAR LOUDSPEAKER + SIGNAL
16 | 1.0 | 34B | LEFT HAND REAR LOUDSPEAKER - SIGNAL