119

| ENGINE WIRING
F4R770,F4R771

#### 119
AUTOMATIC TRANSMISSION COMPUTER
BVA4/TLMEXI BVA4/SSTLMEXI

1 | 1.0 | 5AU | SEQUENCE SOLENOID VALVE +
2 | 0.75 | 5DD | EXCHANGER FLOW SENSOR CONTROL SOLENOID VALVE +
4 | 0.75 | 5CQ | AUTOMATIC GEARBOX DISPLAY SIGNAL
7 | 0.75 | 5AX | SEQUENCE SOLENOID VALVE 3 -
8 | 0.75 | 5AY | SEQUENCE SOLENOID VALVE 4 -
9 | 0.75 | 5AW | SEQUENCE SOLENOID VALVE 2 -
10 | 0.75 | 5AV | SEQUENCE SOLENOID VALVE 1 -
11 | 0.75 | 5DU | GEAR LEVER LOCKING - CONTROL
12 | 0.75 | 5DN | EXCHANGER FLOW SENSOR SOLENOID VALVE - CONTROL
13 | 0.75 | 5DL | MODULATING SOLENOID VALVE 3
14 | 0.75 | 5DM | MODULATING SOLENOID VALVE 4
16 | 0.75 | 5A | BRAKE PEDAL SWITCH + SIGNAL
18 | 0.75 | HK | DIAGNOSTIC SIGNAL K
19 | 1.0 | 5BX | BRIDGING MODULATING SOLENOID VALVE
20 | 1.0 | 5AZ | SEQUENCE SOLENOID VALVE 5 -
24 | 0.75 | 5U | LINE PRESSURE SENSOR +
25 | 0.75 | 5V | LINE PRESSURE SENSOR -
26 | 1.0 | 5BA | MODULATING SOLENOID VALVE +
27 | 2.0 | AP4 | PROTECTED + AFTER IGNITION AUTOMATIC TRANSMISSION FUSE
28 | 2.0 | N | ELECTRONIC EARTH
31 | 0.75 | 5DG | MULTIFUNCTION SWITCH SIGNAL 2
32 | 0.75 | 5DH | MULTIFUNCTION SWITCH SIGNAL 3
33 | 0.75 | 5DJ | MULTIFUNCTION SWITCH SIGNAL 4
36 | 0.75 | 5FM | LOWER CONTACT MULTIFUNCTION PUSH BUTTON CONTROL
37 | 0.75 | 5H | N+1 PUSH BUTTON CONTROL
38 | 0.75 | 3MS | ENGINE CAN H SIGNAL
39 | 0.75 | 3MT | ENGINE CAN L SIGNAL
42 | 0.75 | 5DK | MULTIFUNCTION SWITCH - > AUTOMATIC TRANSMISSION COMPUTER
45 | 0.75 | 5DA | GEARBOX INPUT SPEED SENSOR + SIGNAL
46 | 0.75 | 5DB | GEARBOX INPUT SPEED SENSOR - SIGNAL
53 | 0.75 | 5BC | PRESSURE SOLENOID VALVE 1 -
54 | 0.75 | 5BB | SEQUENCE SOLENOID VALVE 6 -
55 | 0.75 | 5W | LINE PRESSURE SENSOR + SIGNAL
56 | 1.0 | BP42 | PROTECTED + BATTERY FEED > AUTOMATIC TRANSMISSION COMPUTER