R3

| CONNECTION
ANY TYPE

#### R3
DASHBOARD/DRIVER'S DOOR CONNECTION
X84 DD/SUPCPE

6 | 1.0 | 34E | RIGHT HAND FRONT LOUDSPEAKER + SIGNAL
7 | 1.0 | 34F | RIGHT HAND FRONT LOUDSPEAKER - SIGNAL
8 | 0.5 | LPG | PROTECTED LEFT HAND SIDE LIGHT +
11 | 1.4 | 22C | FRONT ELECTRIC WINDOW CONTROL 1
12 | 1.4 | 22D | FRONT ELECTRIC WINDOW CONTROL 2
18 | 2.0 | BP55 | DRIVER'S ONE-TOUCH ELECTRIC WINDOW FUSE PROTECTED + BATTERY FEED
29 | 0.5 | 21K | ANTI-PINCH SUNROOF/ELECTRIC WINDOW SERIAL LINE SIGNAL
30 | 0.35 | 47C | EXTERNAL TEMPERATURE SENSOR + SIGNAL
31 | 0.35 | 47D | EXTERNAL TEMPERATURE SENSOR ZERO VOLTS SIGNAL
39 | 2.0 | MAN | DASHBOARD RIGHT-HAND CROSS MEMBER ELECTRICAL EARTH
40 | 0.5 | 20X | FRONT DEADLOCKING MOTOR CONTROL
41 | 0.35 | 87H | DRIVER'S 1st POSITION SWITCH - SIGNAL
42 | 0.5 | 20BC | DRIVER'S DOOR / FUEL FILLER FLAP UNLOCKING MOTOR CONTROL
42 | 0.5 | 20BC | DRIVER'S DOOR / FUEL FILLER FLAP UNLOCKING MOTOR CONTROL
43 | 0.5 | 20BH | DRIVER'S DOOR / FUEL FILLER FLAP LOCK MOTOR CONTROL
44 | 1.4 | MAN | DASHBOARD RIGHT-HAND CROSS MEMBER ELECTRICAL EARTH
46 | 1.4 | AP30 | PROTECTED + AFTER IGNITION PASSENGER ELECTRIC WINDOW FUSE