239

| DRIVER'S DOOR WIRING
X84

#### 239
DRIVER'S ELECTRIC REAR-VIEW MIRROR
DD/CPE

1 | 0.35 | 15RP | PROTECTED HEATED REAR VIEW MIRROR + CONTROL
2 | 0.35 | 40C | DRIVER'S REAR VIEW MIRROR UP/DOWN CONTROL
3 | 0.35 | 40E | REAR VIEW MIRROR MOTOR COMMON
3 | 0.35 | 40E | REAR VIEW MIRROR MOTOR COMMON
4 | 0.35 | 40A | DRIVER'S REAR VIEW MIRROR RIGHT>LEFT CONTROL
5 | 0.35 | MAN | DASHBOARD RIGHT-HAND CROSS MEMBER ELECTRICAL EARTH
6 | 0.35 | 47C | EXTERNAL TEMPERATURE SENSOR + SIGNAL
7 | 0.35 | 40W | REAR-VIEW MIRROR FOLD IN CONTROL
9 | 0.35 | 40X | REAR-VIEW MIRROR FOLD OUT CONTROL
10 | 0.35 | 47D | EXTERNAL TEMPERATURE SENSOR ZERO VOLTS SIGNAL