261

| DASHBOARD WIRING
DG

#### 261
RADIO
EBASE/SABLAT

1 | 0.35 | 47F | VEHICLE SPEED SIGNAL
4 | 1.0 | BCP3 | PROTECTED + BATTERY FEED CIRCUIT BREAKER INTERIOR LIGHT FUSE
5 | 0.35 | 34AM | WAVE SEPARATOR AERIAL AMPLIFIER +
6 | 0.35 | LPG | PROTECTED LEFT HAND SIDE LIGHT +
7 | 1.0 | SP2 | PROTECTED + ACCESSORIES > RADIO
8 | 3.0 | MAO | DASHBOARD CROSS MEMBER RADIO EARTH
9 | 1.0 | 34D | RIGHT HAND REAR LOUDSPEAKER + SIGNAL
10 | 1.0 | 34C | RIGHT HAND REAR LOUDSPEAKER - SIGNAL
11 | 0.5 | 34E | RIGHT HAND FRONT LOUDSPEAKER + SIGNAL
11 | 1.0 | 34E | RIGHT HAND FRONT LOUDSPEAKER + SIGNAL
12 | 0.5 | 34F | RIGHT HAND FRONT LOUDSPEAKER - SIGNAL
12 | 1.0 | 34F | RIGHT HAND FRONT LOUDSPEAKER - SIGNAL
13 | 0.5 | 34G | LEFT HAND FRONT LOUDSPEAKER + SIGNAL
13 | 1.0 | 34G | LEFT HAND FRONT LOUDSPEAKER + SIGNAL
14 | 0.5 | 34H | LEFT HAND FRONT LOUDSPEAKER - SIGNAL
14 | 1.0 | 34H | LEFT HAND FRONT LOUDSPEAKER - SIGNAL
15 | 1.0 | 34A | LEFT HAND REAR LOUDSPEAKER + SIGNAL
16 | 1.0 | 34B | LEFT HAND REAR LOUDSPEAKER - SIGNAL