1337

| ENGINE WIRING
K9K722

#### 1337
SWITCHING PROTECTION UNIT
CA,CAREG/SANFLT CA,CAREG/FLTDIE

2 | 0.5 | 3AA | INJECTION LOCKING RELAY COIL - CONTROL
3 | 0.5 | 2K | ALTERNATOR CHARGER SIGNAL
6 | 0.5 | 26Z | AUTOMATIC TRANSMISSION NEUTRAL + SIGNAL
8 | 0.5 | 2JD | ALTERNATOR FEED +
10 | 0.5 | 32B | OIL LEVEL SENSOR SIGNAL 1
11 | 0.5 | 32A | OIL LEVEL SENSOR SIGNAL 2
12 | 0.5 | 28A | OIL PRESSURE WARNING LIGHT - CONTROL