120

| ENGINE WIRING
F4R770,F4R771

#### 120
INJECTION COMPUTER
BVA4/TLMEXI BVM6 BVA4/SSTLMEXI

B1 | 0.75 | 3GK | UPSTREAM OXYGEN SENSOR SIGNAL
C1 | 0.75 | 3GH | UPSTREAM OXYGEN SENSOR EARTH
D1 | 0.5 | 3AC | FUEL PUMP RELAY COIL - CONTROL
E1 | 0.5 | 3BB | CANISTER BLEED SOLENOID VALVE
L1 | 1.4 | N | ELECTRONIC EARTH
M1 | 1.4 | N | ELECTRONIC EARTH
A2 | 0.75 | 3GL | DOWNSTREAM OXYGEN SENSOR SIGNAL
B2 | 0.75 | 3GJ | DOWNSTREAM OXYGEN SENSOR EARTH
L2 | 1.0 | 3GF | UPSTREAM OXYGEN SENSOR HEATER - CONTROL
L3 | 1.0 | 3GG | DOWNSTREAM OXYGEN SENSOR HEATER - CONTROL
M3 | 1.0 | 3CW | INJECTOR 2 & 3 IGNITION COIL - CONTROL
M4 | 1.0 | 3CV | INJECTOR 1 & 4 IGNITION COIL - CONTROL