R2

| CONNECTION
ANY TYPE

#### R2
DASHBOARD/LEFT REAR CONNECTION
X84 B84,S84/DG/SPRGAZ/EPACK X84 B84,S84/DG/EQGPL/EPACK

31 | 0.5 | 4G | LEFT HAND REAR WHEEL SENSOR SIGNAL
32 | 0.5 | 4H | LEFT HAND REAR WHEEL SENSOR +
33 | 0.5 | 4S | RIGHT HAND REAR WHEEL SENSOR SIGNAL
34 | 0.5 | 4T | RIGHT HAND REAR WHEEL SENSOR +
35 | 3.0 | 15LP | PROTECTED HEATED REAR SCREEN + CONTROL
40 | 1.0 | 34A | LEFT HAND REAR LOUDSPEAKER + SIGNAL
41 | 1.0 | 34B | LEFT HAND REAR LOUDSPEAKER - SIGNAL
42 | 1.0 | 34C | RIGHT HAND REAR LOUDSPEAKER - SIGNAL
43 | 1.0 | 34D | RIGHT HAND REAR LOUDSPEAKER + SIGNAL
44 | 0.35 | 34AM | WAVE SEPARATOR AERIAL AMPLIFIER +
51 | 0.5 | 41A | FUEL LEVEL SENDER + SIGNAL
52 | 0.5 | 41B | FUEL LEVEL -
1 | 1.0 | BPR1 | + BATTERY FEED > RELAY
1 | 1.0 | BPR1 | + BATTERY FEED > RELAY
2 | 0.5 | 103A | HEADLIGHT POSITION CONTROL
3 | 0.5 | CPD | PROTECTED RIGHT HAND DIPPED BEAM HEADLIGHT +
6 | 0.35 | 79K | LEFT HAND HEATED SEAT RELAY + CONTROL
7 | 0.35 | 79L | RIGHT HAND HEATED SEAT RELAY + CONTROL
8 | 0.5 | SP2 | PROTECTED + ACCESSORIES > RADIO
8 | 0.5 | SP2 | PROTECTED + ACCESSORIES > RADIO
36 | 0.35 | 3RD | LIQUEFIED PETROLEUM GAS GAUGE SENDER SIGNAL
37 | 0.35 | 3XC | - NATURAL GAS PRESSURE SENSOR URBAN DRIVING
38 | 1.4 | 3VK | LPG TANK SOLENOID VALVE CONTROL
39 | 0.35 | 3YB | LIQUID PETROLEUM GAS GAUGE 5 V SIGNAL
5 | 0.5 | 9P | PROTECTED REAR FOG LIGHTS + CONTROL
4 | 1.4 | 3N | FUEL PUMP +
9 | 0.5 | LPD | PROTECTED RIGHT HAND SIDE LIGHT +
9 | 0.5 | LPD | PROTECTED RIGHT HAND SIDE LIGHT +
10 | 0.75 | LPG | PROTECTED LEFT HAND SIDE LIGHT +
11 | 0.75 | 65A | BRAKE LIGHTS + CONTROL
12 | 0.5 | 64C | LEFT HAND TURN SIGNAL LIGHTS CONTROL
13 | 0.5 | 64D | RIGHT HAND TURN SIGNAL LIGHTS CONTROL
14 | 0.5 | H66P | REVERSING LIGHTS + CONTROL
14 | 0.5 | H66P | REVERSING LIGHTS + CONTROL
15 | 0.5 | 9P | PROTECTED REAR FOG LIGHTS + CONTROL
16 | 0.5 | 20S | TAILGATE MOTOR OPENING AUTHORISED FEED
17 | 0.35 | 87A | LEFT HAND REAR 1st POSITION SWITCH - SIGNAL
18 | 0.35 | 87B | RIGHT HAND REAR 1st POSITION SWITCH - SIGNAL
19 | 0.5 | 87T | BOOT LID POSITION SWITCH 1 SIGNAL
20 | 0.5 | 20BH | DRIVER'S DOOR / FUEL FILLER FLAP LOCK MOTOR CONTROL
21 | 0.5 | 20BC | DRIVER'S DOOR / FUEL FILLER FLAP UNLOCKING MOTOR CONTROL
22 | 0.5 | 20BK | PASSENGER DOORS / REAR DOORS LOCKING MOTOR CONTROL
22 | 0.5 | 20BK | PASSENGER DOORS / REAR DOORS LOCKING MOTOR CONTROL
23 | 0.5 | 20G | TAILGATE MOTOR OPEN CONTROL
24 | 0.5 | 20BD | OPEN FRONT/REAR PASSENGER DOORS MOTOR CONTROL
24 | 0.5 | 20BD | OPEN FRONT/REAR PASSENGER DOORS MOTOR CONTROL
25 | 0.35 | 20BG | REAR DOORS DEADLOCKING STATUS SIGNAL
25 | 0.35 | 20BG | REAR DOORS DEADLOCKING STATUS SIGNAL
26 | 0.5 | 20W | REAR DEADLOCKING MOTOR CONTROL
26 | 0.5 | 20W | REAR DEADLOCKING MOTOR CONTROL
27 | 0.35 | BPT | PROTECTED + BATTERY FEED TIMER
28 | 0.35 | 13E | INTERIOR LIGHTS - CONTROL > TIMER
29 | 1.0 | 36A | REAR WIPER + CONTROL
30 | 0.35 | 36C | REAR SCREEN WIPER PARK POSITION SWITCH - SIGNAL