120

| ENGINE WIRING
K4J730,K4M764

#### 120
INJECTION COMPUTER
K4J730/CHAUFO K4J730/CA,CAREG K4M764/EQGPL

C3 | 0.5 | H7 | REV COUNTER > TOP DEAD CENTRE > COIL > COMPUTER ALTERNATOR SIGNAL
K3 | 0.5 | 3MT | ENGINE CAN L SIGNAL
K4 | 0.5 | 3MS | ENGINE CAN H SIGNAL
A1 | 0.75 | 3CR | INJECTOR 1 - CONTROL
L1 | 1.4 | N | ELECTRONIC EARTH
M1 | 1.4 | N | ELECTRONIC EARTH
A2 | 0.75 | 3CS | INJECTOR 2 - CONTROL
B2 | 0.5 | TB1 | PINKING SENSOR SCREENING BRAID
E2 | 0.5 | 3B | AIR TEMPERATURE SENSOR + SIGNAL
F2 | 0.75 | 3C | COOLANT TEMPERATURE SENSOR + SIGNAL
G2 | 0.5 | 3MN | MOTORISED THROTTLE POTENTIOMETER + 5 VOLTS
H2 | 0.5 | 3LG | ATMOSPHERIC PRESSURE SENSOR +
M2 | 1.4 | 3FB1 | INJECTION + > PROTECTIVE RELAY
A3 | 0.75 | 3CT | INJECTOR 3 - CONTROL
B3 | 0.5 | 3S | PINKING SENSOR 1 + SIGNAL > FRONT
D3 | 0.5 | 3MQ | MOTORISED THROTTLE POTENTIOMETER 2 SIGNAL
E3 | 0.5 | 3JQ | AIR TEMPERATURE -
F3 | 0.75 | 3BG | ENGINE SPEED SIGNAL > TDC SENSOR
G3 | 0.5 | 3MP | MOTORISED THROTTLE POTENTIOMETER 1 SIGNAL
H3 | 0.5 | 3F | ATMOSPHERIC PRESSURE SENSOR SIGNAL
M3 | 1.4 | 3AJB | THROTTLE MOTOR + CONTROL
A4 | 0.75 | 3CU | INJECTOR 4 - CONTROL
B4 | 0.5 | 3DQ | PINKING SENSOR -
D4 | 0.5 | 3AA | INJECTION LOCKING RELAY COIL - CONTROL
E4 | 0.75 | 3BL | ENGINE SPEED > TDC SENSOR - SIGNAL
F4 | 0.75 | 3JK | COOLANT TEMPERATURE -
G4 | 0.5 | 3MO | MOTORISED THROTTLE POTENTIOMETER SENSOR -
H4 | 0.5 | 3CK | UNIT 2 SENSOR -
M4 | 1.4 | 3AJC | THROTTLE MOTOR - CONTROL
J2 | 0.75 | 38Y | REFRIGERANT GAS PRESSURE SENSOR +
K2 | 0.75 | 38U | RHEOSTAT CURSOR
J3 | 0.75 | 38X | REFRIGERANT GAS PRESSURE SENSOR SIGNAL