R341

| CONNECTION
ANY TYPE

#### R341
DRIVER'S SEAT / FLOOR
X84 B84,S84/DD/EQGPL

3 | 0.35 | 60CL | DRIVER'S SEAT POSITION EARTH
4 | 0.35 | 60BP | DRIVER'S SEAT POSITION SIGNAL
5 | 0.35 | 60DU | DRIVER'S SEATBELT WARNING SIGNAL
6 | 0.35 | 60DV | DRIVER'S SEATBELT WARNING EARTH
7 | 0.35 | 60D | DRIVER'S PRETENSIONER + SIGNAL
8 | 0.35 | 60E | DRIVER'S PRETENSIONER - SIGNAL
9 | 0.35 | 60AK | DRIVER'S LAP STRAP PRETENSIONER + CONTROL
10 | 0.35 | 60AL | DRIVER'S LAP STRAP PRETENSIONER - CONTROL
11 | 0.35 | 60AR | DRIVER'S SIDE THORAX AIR BAG + CONTROL
12 | 0.35 | 60AS | - DRIVER'S SIDE THORAX AIR BAG CONTROL
13 | 0.35 | MAQ | REAR RIGHT-HAND END PANEL ELECTRICAL EARTH
19 | 0.35 | 79L | RIGHT HAND HEATED SEAT RELAY + CONTROL
20 | 0.5 | SP2 | PROTECTED + ACCESSORIES > RADIO
21 | 1.0 | BPR1 | + BATTERY FEED > RELAY
22 | 1.0 | MAQ | REAR RIGHT-HAND END PANEL ELECTRICAL EARTH