662

| RADIO/MULTIMEDIA DISPLAY INTERMEDIATE WIRING
DG

#### 662
NAVIGATION COMPUTER
RAD03/NINAV3

1 | 0.5 | BCP3 | PROTECTED + BATTERY FEED CIRCUIT BREAKER INTERIOR LIGHT FUSE
3 | 0.35 | 46AZ | NAVIGATION AUDIO + SIGNAL
6 | 0.35 | 46AD | NAVIGATION ON/OFF CONTROL
7 | 0.22 | 46BL | NAVIGATION SHUNT H SIGNAL
8 | 0.22 | 46BL | NAVIGATION SHUNT H SIGNAL
9 | 0.35 | 46BB | NAVIGATION CAN H SIGNAL 1
10 | 0.5 | MAN | DASHBOARD RIGHT-HAND CROSS MEMBER ELECTRICAL EARTH
12 | 0.35 | 46BA | NAVIGATION AUDIO - SIGNAL
15 | 0.35 | 47F | VEHICLE SPEED SIGNAL
16 | 0.22 | 46BM | NAVIGATION SHUNT L SIGNAL
17 | 0.22 | 46BM | NAVIGATION SHUNT L SIGNAL
18 | 0.35 | 46BC | NAVIGATION CAN L SIGNAL