1107

| DASHBOARD WIRING
DD

#### 1107
CLUSTER SENSOR
ANY TYPE

1 | 0.5 | 4CV | YAW SENSOR REFERENCE SIGNAL (DIRECTIONAL STABILITY)
2 | 0.5 | 4BZ | YAW SENSOR TEST SIGNAL (DIRECTIONAL STABILITY)
3 | 0.5 | SP15 | PROTECTED + ACCESSORIES FEED FUSE
4 | 0.5 | 4CW | YAW SENSOR SIGNAL (DIRECTIONAL STABILITY)
5 | 0.5 | 4CX | LATERAL ACCELERATION SENSOR SIGNAL
6 | 0.5 | 4CY | YAW SENSOR - (DIRECTIONAL STABILITY) > LATERAL ACCELERATION