120

| ENGINE WIRING
F9Q800,F9Q808

#### 120
INJECTION COMPUTER
F9Q800/SANFLT F9Q808 F9Q800/FLTDIE

E1 | 0.5 | 3MG | TURBO PRESSURE SOLENOID VALVE - CONTROL
F1 | 0.5 | 3LD | FUEL TEMPERATURE SENSOR -
G1 | 2.0 | 3KZ | INJECTOR 4 CONTROL
H1 | 2.0 | 3KW | INJECTOR 1 CONTROL
C2 | 0.5 | 3JM | EGR SOLENOID VALVE -
E2 | 0.5 | 3FF | PRE-HEATER RELAY - CONTROL
G2 | 2.0 | 3KX | INJECTOR 2 CONTROL
H2 | 2.0 | 3KY | INJECTOR 3 CONTROL
C3 | 0.75 | 38U | RHEOSTAT CURSOR
G3 | 2.0 | 3CR | INJECTOR 1 - CONTROL
H3 | 2.0 | 3CU | INJECTOR 4 - CONTROL
A4 | 0.5 | 3FY | PRE-HEATER RELAY DIAGNOSTIC SIGNAL
G4 | 2.0 | 3CS | INJECTOR 2 - CONTROL
H4 | 2.0 | 3CT | INJECTOR 3 - CONTROL
A2 | 0.5 | 3WT | WATER IN DIESEL DETECTION SENSOR SIGNAL