1094

| DASHBOARD WIRING
DD

#### 1094
ANTI-LOCK BRAKING SYSTEM/ELECTRONIC STABILITY PROGRAM COMPUTER
ANY TYPE

1 | 4.0 | MAH | ANTI-LOCK BRAKING SYSTEM ELECTRICAL EARTH
2 | 4.0 | BP8 | PROTECTED + BATTERY FEED > ANTI-LOCK BRAKING SYSTEM MOTOR
3 | 2.5 | BP14 | PROTECTED + BATTERY FEED > ABS
4 | 2.5 | MAH | ANTI-LOCK BRAKING SYSTEM ELECTRICAL EARTH
5 | 0.5 | 4C | LEFT HAND FRONT WHEEL SENSOR SIGNAL
6 | 0.5 | 4H | LEFT HAND REAR WHEEL SENSOR +
8 | 0.5 | 4T | RIGHT HAND REAR WHEEL SENSOR +
9 | 0.5 | 4N | RIGHT HAND FRONT WHEEL SENSOR +
10 | 0.5 | 4M | RIGHT HAND FRONT WHEEL SENSOR SIGNAL
11 | 0.75 | HK | DIAGNOSTIC SIGNAL K
14 | 0.5 | 4DN | ANTI-LOCK BRAKING SYSTEM LOWER CAN SIGNAL
15 | 0.5 | 4CY | YAW SENSOR - (DIRECTIONAL STABILITY) > LATERAL ACCELERATION
16 | 0.5 | 4CW | YAW SENSOR SIGNAL (DIRECTIONAL STABILITY)
18 | 0.5 | 4CV | YAW SENSOR REFERENCE SIGNAL (DIRECTIONAL STABILITY)
20 | 0.5 | 4CX | LATERAL ACCELERATION SENSOR SIGNAL
22 | 0.5 | 4GJ | BRAKE LIGHTS ON CONTROL RELAY
26 | 0.5 | 4E | LEFT HAND FRONT WHEEL SENSOR +
27 | 0.5 | 4G | LEFT HAND REAR WHEEL SENSOR SIGNAL
28 | 0.75 | SP15 | PROTECTED + ACCESSORIES FEED FUSE
29 | 0.5 | 4S | RIGHT HAND REAR WHEEL SENSOR SIGNAL
30 | 0.75 | 65G | BRAKE LIGHT CONTROL > RELAY
31 | 0.5 | 4AQ | ELECTRONIC STABILITY PROGRAM ON/OFF SWITCH - CONTROL
33 | 0.75 | 47F | VEHICLE SPEED SIGNAL
35 | 0.5 | 4DM | ANTI-LOCK BRAKING SYSTEM UPPER CAN SIGNAL
37 | 0.5 | 4BZ | YAW SENSOR TEST SIGNAL (DIRECTIONAL STABILITY)