1088

| DASHBOARD WIRING
DG

#### 1088
STEERING COLUMN ELECTRIC LOCK
EBASE/ABLAV EBASE/SABLAT CA,CAREG/SSESP CA,CAREG/ASRESP

1 | 0.5 | NAM | UPPER LEFT-HAND CROSS MEMBER ELECTRONIC EARTH
2 | 0.35 | 26I | + STEERING COLUMN LOCK
3 | 0.35 | 26AZ | KEYLESS VEHICLE STEERING COLUMN LOCK CAN H SIGNAL
4 | 0.35 | 26J | CONTROL - SAFETY HALL SENSOR
5 | 0.35 | AP15 | PROTECTED + AFTER IGNITION ENGINE FUNCTIONS FUSE
6 | 0.35 | 26BA | KEYLESS VEHICLE STEERING COLUMN LOCK CAN L SIGNAL