R3

| CONNECTION
ANY TYPE

#### R3
DASHBOARD/DRIVER'S DOOR CONNECTION
X84 DD/CPE

1 | 0.5 | BCP3 | PROTECTED + BATTERY FEED CIRCUIT BREAKER INTERIOR LIGHT FUSE
2 | 0.35 | BPT2 | + BATTERY PROTECTED TIMED LIGHTING
3 | 0.35 | 13AC | FOOTWELL LIGHTING TIMER + CONTROL
4 | 0.35 | 20AL | REAR INTERIOR LOCKING CONTROL
5 | 0.35 | 20T | CHILD SAFETY LED - CONTROL
6 | 1.0 | 34E | RIGHT HAND FRONT LOUDSPEAKER + SIGNAL
7 | 1.0 | 34F | RIGHT HAND FRONT LOUDSPEAKER - SIGNAL
8 | 0.5 | LPG | PROTECTED LEFT HAND SIDE LIGHT +
9 | 0.35 | 22A | PASSENGER'S ELECTRIC WINDOW UP CONTROL
10 | 0.35 | 22B | PASSENGER'S ELECTRIC WINDOW DOWN CONTROL
11 | 0.35 | 22C | FRONT ELECTRIC WINDOW CONTROL 1
12 | 0.35 | 22D | FRONT ELECTRIC WINDOW CONTROL 2
13 | 0.35 | 23A | ELECTRIC WINDOW CONTROL > RIGHT-HAND REAR QUARTER LIGHT CLOSE
14 | 0.35 | 23B | ELECTRIC WINDOW DOWN CONTROL > RIGHT HAND REAR QUARTER LIGHT OPEN
15 | 0.35 | 23C | ELECTRIC WINDOW UP CONTROL > LEFT HAND REAR QUARTER LIGHT CLOSE
16 | 0.35 | 23D | ELECTRIC WINDOW DOWN CONTROL > LEFT HAND REAR QUARTER LIGHT OPEN
17 | 0.35 | 23G | RIGHT HAND REAR ELECTRIC WINDOW CONTROL 1
18 | 2.0 | BP55 | DRIVER'S ONE-TOUCH ELECTRIC WINDOW FUSE PROTECTED + BATTERY FEED
19 | 0.35 | 23H | RIGHT HAND REAR ELECTRIC WINDOW CONTROL 2
20 | 0.35 | 23J | LEFT HAND REAR ELECTRIC WINDOW CONTROL 1
21 | 0.35 | 23K | LEFT HAND REAR ELECTRIC WINDOW CONTROL 2
22 | 0.35 | 40B | PASSENGER REAR VIEW MIRROR UP/DOWN CONTROL
23 | 0.35 | 40D | PASSENGER REAR VIEW MIRROR RIGHT>LEFT CONTROL
24 | 0.35 | 40E | REAR VIEW MIRROR MOTOR COMMON
25 | 0.35 | 40X | REAR-VIEW MIRROR FOLD OUT CONTROL
25 | 0.35 | 40X | REAR-VIEW MIRROR FOLD OUT CONTROL
26 | 0.35 | 40W | REAR-VIEW MIRROR FOLD IN CONTROL
26 | 0.35 | 40W | REAR-VIEW MIRROR FOLD IN CONTROL
28 | 0.35 | 15RP | PROTECTED HEATED REAR VIEW MIRROR + CONTROL
29 | 0.5 | 21K | ANTI-PINCH SUNROOF/ELECTRIC WINDOW SERIAL LINE SIGNAL
30 | 0.35 | 47C | EXTERNAL TEMPERATURE SENSOR + SIGNAL
31 | 0.35 | 47D | EXTERNAL TEMPERATURE SENSOR ZERO VOLTS SIGNAL
33 | 0.5 | 26P | DOOR HANDLE INFRARED SENSOR +
34 | 0.35 | 26AP | KEYLESS VEHICLE LOCKING SIGNAL / DRIVER SIDE DOORS SWITCH
35 | 0.5 | 26T | DRIVER'S HANDLE INFRARED SENSOR SIGNAL
37 | 0.35 | 26AA | KEYLESS VEHICLE DRIVER'S FRONT DOOR EXTERNAL AERIAL A SIGNAL
38 | 0.35 | 26AB | KEYLESS VEHICLE DRIVER'S SIDE FRONT DOOR EXTERNAL AERIAL B SIGNAL
39 | 2.0 | MAN | DASHBOARD RIGHT-HAND CROSS MEMBER ELECTRICAL EARTH
41 | 0.5 | 87H | DRIVER'S 1st POSITION SWITCH - SIGNAL
42 | 0.5 | 20BC | DRIVER'S DOOR / FUEL FILLER FLAP UNLOCKING MOTOR CONTROL
43 | 0.5 | 20BH | DRIVER'S DOOR / FUEL FILLER FLAP LOCK MOTOR CONTROL
45 | 0.35 | BPT | PROTECTED + BATTERY FEED TIMER