R4

| CONNECTION
ANY TYPE

#### R4
DASHBOARD/PASSENGER'S DOOR CONNECTION
DG CA,CAREG/SSESP DG CA,CAREG/ASRESP

2 | 0.35 | BPT2 | + BATTERY PROTECTED TIMED LIGHTING
3 | 0.35 | 13AC | FOOTWELL LIGHTING TIMER + CONTROL
4 | 0.35 | 47C | EXTERNAL TEMPERATURE SENSOR + SIGNAL
5 | 0.35 | 47D | EXTERNAL TEMPERATURE SENSOR ZERO VOLTS SIGNAL
6 | 1.0 | 34E | RIGHT HAND FRONT LOUDSPEAKER + SIGNAL
7 | 1.0 | 34F | RIGHT HAND FRONT LOUDSPEAKER - SIGNAL
8 | 0.5 | LPG | PROTECTED LEFT HAND SIDE LIGHT +
9 | 0.35 | 22A | PASSENGER'S ELECTRIC WINDOW UP CONTROL
10 | 0.35 | 22B | PASSENGER'S ELECTRIC WINDOW DOWN CONTROL
11 | 0.35 | 22C | FRONT ELECTRIC WINDOW CONTROL 1
12 | 0.35 | 22D | FRONT ELECTRIC WINDOW CONTROL 2
18 | 2.0 | BP70 | PROTECTED + BATTERY FEED > PASSENGER'S ONE-TOUCH FRONT ELECTRIC WINDOW FUSE
22 | 0.35 | 40B | PASSENGER REAR VIEW MIRROR UP/DOWN CONTROL
23 | 0.35 | 40D | PASSENGER REAR VIEW MIRROR RIGHT>LEFT CONTROL
24 | 0.35 | 40E | REAR VIEW MIRROR MOTOR COMMON
25 | 0.35 | 40X | REAR-VIEW MIRROR FOLD OUT CONTROL
26 | 0.35 | 40W | REAR-VIEW MIRROR FOLD IN CONTROL
28 | 0.35 | 15RP | PROTECTED HEATED REAR VIEW MIRROR + CONTROL
29 | 0.35 | 21K | ANTI-PINCH SUNROOF/ELECTRIC WINDOW SERIAL LINE SIGNAL
33 | 0.5 | 26P | DOOR HANDLE INFRARED SENSOR +
34 | 0.35 | 26AQ | KEYLESS VEHICLE LOCKING SIGNAL / PASSENGER SIDE DOORS SWITCH
35 | 0.35 | 26Q | PASSENGER SIDE DOOR HANDLE INFRARED SENSOR SIGNAL
37 | 0.35 | 26AC | KEYLESS VEHICLE FRONT PASSENGER DOOR EXTERNAL AERIAL A SIGNAL
38 | 0.35 | 26AD | KEYLESS VEHICLE FRONT RIGHT DOOR EXTERNAL AERIAL SIGNAL 2
39 | 3.0 | MAN | DASHBOARD RIGHT-HAND CROSS MEMBER ELECTRICAL EARTH
40 | 0.5 | 20BK | PASSENGER DOORS / REAR DOORS LOCKING MOTOR CONTROL
41 | 0.5 | 20BD | OPEN FRONT/REAR PASSENGER DOORS MOTOR CONTROL
42 | 0.22 | 87G | PASSENGER'S 1st POSITION SWITCH - SIGNAL