1550

| ENGINE WIRING
F9Q804

#### 1550
ADDITIONAL HEATER UNIT INTERFACE
ANY TYPE

1 | 2.5 | 3JB | ADDITIONAL HEATER PLUG 1 + CONTROL
2 | 0.5 | 3JAA | ADDITIONAL HEATER 2 RELAY COIL CONTROL
3 | 2.5 | 3JD | ADDITIONAL HEATER PLUG 3 + CONTROL
4 | 5.0 | BP27 | PROTECTED + BATTERY FEED > ENGINE FUNCTIONS
5 | 5.0 | BP35 | PROTECTED + BATTERY FEED PRE-HEATER UNIT FUSE
6 | 0.5 | 3JA | ADDITIONAL HEATER 1 RELAY COIL CONTROL
7 | 2.5 | 3JC | ADDITIONAL HEATER PLUG 2 + CONTROL
8 | 0.5 | HK8 | ADDITIONAL HEATER DIAGNOSTIC SIGNAL