R301

| CONNECTION
ANY TYPE

#### R301
DASHBOARD/COURTESY LIGHT CONNECTION
TN PRETEL/EBASE TN PRETEL/EPACK TOELEC/TOELEF -

11 | 0.35 | 107G | HANDS FREE TELEPHONE MICROPHONE +
12 | 0.35 | 107H | HANDS FREE TELEPHONE MICROPHONE -
1 | 0.35 | AP1A | ROOF FUSE PROTECTED + AFTER IGNITION
2 | 0.35 | 14S | RAIN SENSOR SERIAL LINE SIGNAL
3 | 0.35 | MAM | DASHBOARD LEFT-HAND CROSS MEMBER ELECTRICAL EARTH
4 | 0.35 | MAM | DASHBOARD LEFT-HAND CROSS MEMBER ELECTRICAL EARTH
5 | 0.35 | XXXX | EMPTY CONNECTION
6 | 0.35 | AP1A | ROOF FUSE PROTECTED + AFTER IGNITION
7 | 0.35 | 38GZ | INTERIOR TEMPERATURE SENSOR SIGNAL
8 | 0.35 | 38JN | SUN TEMPERATURE HUMIDITY SENSOR ZERO VOLTS
9 | 0.35 | MAM | DASHBOARD LEFT-HAND CROSS MEMBER ELECTRICAL EARTH
10 | 0.35 | AP1A | ROOF FUSE PROTECTED + AFTER IGNITION