139

| LEFT-HAND REAR DOOR WIRING
B84,S84

#### 139
REAR LEFT DOOR ELECTRIC LOCKING
EPACK EPACKP SUPCPE/EBASE

A | 0.5 | 20BK | PASSENGER DOORS / REAR DOORS LOCKING MOTOR CONTROL
B | 0.5 | 20BD | OPEN FRONT/REAR PASSENGER DOORS MOTOR CONTROL
C | 0.5 | 87A | LEFT HAND REAR 1st POSITION SWITCH - SIGNAL
D | 0.5 | MZ | REAR END PANEL ELECTRICAL EARTH
E | 0.5 | 20W | REAR DEADLOCKING MOTOR CONTROL
F | 0.5 | 20BG | REAR DOORS DEADLOCKING STATUS SIGNAL