645

| DASHBOARD WIRING
DG

#### 645
PASSENGER COMPARTMENT COMPUTER
EBASE/ABLAV CA,CAREG/ASRESP

21 | 0.35 | 26BH | + CARD READER
22 | 0.35 | 38JV | PASSENGER COMPARTMENT HEATING RESISTANCE CONTROL RELAY 2PASSENGER
24 | 0.35 | 15M | HEATED REAR SCREEN RELAY - CONTROL
25 | 0.35 | 26BK | - CARD READER
26 | 0.35 | 38ES | AIR CONDITIONING WARNING LIGHT - CONTROL
27 | 0.75 | 65G | BRAKE LIGHT CONTROL > RELAY
28 | 0.5 | 24A | REAR SCREEN WASHER PUMP + CONTROL
29 | 0.35 | 80T | ENGINE IMMOBILISER WARNING LIGHT - CONTROL
30 | 0.35 | 38LP | AIR CONDITIONING STOP/START CONTROL
32 | 0.35 | 38LQ | FAN ASSEMBLY SPEED 0 SIGNAL
33 | 0.35 | 38JU | PASSENGER COMPARTMENT HEATING RESISTANCE CONTROL RELAY 1
34 | 0.5 | S | + ACCESSORIES FEED
35 | 0.35 | 64Q | FLASHER UNIT TIMER - CONTROL
36 | 0.35 | 5A | BRAKE PEDAL SWITCH + SIGNAL
37 | 0.22 | 36C | REAR SCREEN WIPER PARK POSITION SWITCH - SIGNAL
38 | 0.35 | 15A | HEATED REAR SCREEN WARNING LIGHT CONTROL
39 | 0.35 | 26BG | UCH DATA / CARD READER SIGNAL
40 | 0.35 | 26BD | UCH SYNCHRONISATION / CARD READER SIGNAL