645

| DASHBOARD WIRING
DG

#### 645
PASSENGER COMPARTMENT COMPUTER
EBASE/ABLAV EBASE/SABLAT CA,CAREG/SSESP CA,CAREG/ASRESP

1 | 0.35 | 26I | + STEERING COLUMN LOCK
2 | 1.4 | APCB | + AFTER IGNITION PROTECTED / COLUMN LOCK FUSE CONTACT CLOSED AT REST
3 | 1.0 | 36A | REAR WIPER + CONTROL
4 | 1.4 | BP25 | PROTECTED + BATTERY FEED REAR SCREEN WIPER
5 | 0.5 | 20BH | DRIVER'S DOOR / FUEL FILLER FLAP LOCK MOTOR CONTROL
5 | 0.5 | 20BH | DRIVER'S DOOR / FUEL FILLER FLAP LOCK MOTOR CONTROL
6 | 0.5 | 20BC | DRIVER'S DOOR / FUEL FILLER FLAP UNLOCKING MOTOR CONTROL
6 | 0.5 | 20BC | DRIVER'S DOOR / FUEL FILLER FLAP UNLOCKING MOTOR CONTROL
7 | 0.5 | 20BK | PASSENGER DOORS / REAR DOORS LOCKING MOTOR CONTROL
7 | 1.0 | 20BK | PASSENGER DOORS / REAR DOORS LOCKING MOTOR CONTROL
8 | 0.5 | 20BD | OPEN FRONT/REAR PASSENGER DOORS MOTOR CONTROL
8 | 1.0 | 20BD | OPEN FRONT/REAR PASSENGER DOORS MOTOR CONTROL
9 | 2.0 | BP3 | PROTECTED + BATTERY FEED ELECTRIC DOOR LOCKING
11 | 1.0 | 20W | REAR DEADLOCKING MOTOR CONTROL