R4

| CONNECTION
ANY TYPE

#### R4
DASHBOARD/PASSENGER'S DOOR CONNECTION
X84 B84,S84/DD/SUPCPE

6 | 1.0 | 34G | LEFT HAND FRONT LOUDSPEAKER + SIGNAL
7 | 1.0 | 34H | LEFT HAND FRONT LOUDSPEAKER - SIGNAL
8 | 0.5 | LPG | PROTECTED LEFT HAND SIDE LIGHT +
11 | 1.4 | 22C | FRONT ELECTRIC WINDOW CONTROL 1
12 | 1.4 | 22D | FRONT ELECTRIC WINDOW CONTROL 2
39 | 3.0 | MAM | DASHBOARD LEFT-HAND CROSS MEMBER ELECTRICAL EARTH
40 | 0.5 | 20BK | PASSENGER DOORS / REAR DOORS LOCKING MOTOR CONTROL
41 | 0.5 | 20BD | OPEN FRONT/REAR PASSENGER DOORS MOTOR CONTROL
42 | 0.35 | 87G | PASSENGER'S 1st POSITION SWITCH - SIGNAL
43 | 0.5 | 20BC | DRIVER'S DOOR / FUEL FILLER FLAP UNLOCKING MOTOR CONTROL
44 | 0.5 | 20X | FRONT DEADLOCKING MOTOR CONTROL