120

| ENGINE WIRING
K9K728,K9K729

#### 120
INJECTION COMPUTER
K9K728/CHAUFO/SANFLT K9K728/CA,CAREG/SANFLT K9K728/CHAUFO/FLTDIE

A1 | 0.5 | 3KJ | AIRFLOW +
B1 | 0.5 | 3GC | EGR SENSOR +
C1 | 0.5 | 3LQ | TURBOCHARGER PRESSURE SENSOR +
D1 | 0.5 | 3LX | RAIL FUEL PRESSURE SENSOR +
F1 | 0.5 | 3DQ | PINKING SENSOR -
G1 | 0.5 | 3S | PINKING SENSOR 1 + SIGNAL > FRONT
K1 | 0.5 | TB1 | PINKING SENSOR SCREENING BRAID
A2 | 0.5 | 3DV | AIRFLOW SENSOR + SIGNAL
B2 | 0.5 | 3EL | EGR POTENTIOMETER + SIGNAL
C2 | 0.5 | 3LP | TURBOCHARGER PRESSURE SENSOR + SIGNAL
D2 | 0.5 | 3LY | RAIL FUEL PRESSURE SENSOR + SIGNAL
E2 | 0.5 | 3CQ | CAMSHAFT SENSOR SIGNAL
F2 | 0.5 | 3BG | ENGINE SPEED SIGNAL > TDC SENSOR
G2 | 0.5 | 3FAB | FUEL TEMPERATURE + SIGNAL
H2 | 0.5 | 3C | COOLANT TEMPERATURE SENSOR + SIGNAL
J2 | 0.5 | 3KQ | AIR TEMPERATURE SIGNAL
K2 | 0.5 | 3B | AIR TEMPERATURE SENSOR + SIGNAL
M2 | 0.75 | 3MG | TURBO PRESSURE SOLENOID VALVE - CONTROL
A3 | 0.5 | 3DW | AIRFLOW SENSOR - SIGNAL
B3 | 0.5 | 3JM | EGR SOLENOID VALVE -
C3 | 0.5 | 3LN | TURBOCHARGER PRESSURE SENSOR -
D3 | 0.5 | 3LZ | RAIL FUEL PRESSURE SENSOR -
E3 | 0.5 | 3PL | BANK A>B CAMSHAFT SENSOR EARTH
F3 | 0.5 | 3BL | ENGINE SPEED > TDC SENSOR - SIGNAL
G3 | 0.5 | 3LD | FUEL TEMPERATURE SENSOR -
H3 | 0.5 | 3JK | COOLANT TEMPERATURE -
L3 | 0.75 | 3GB | EGR SOLENOID VALVE -
A4 | 0.75 | 3L | + INJECTOR 1
B4 | 0.75 | 3KW | INJECTOR 1 CONTROL
C4 | 0.75 | 3LB | + INJECTOR 3
D4 | 0.75 | 3KY | INJECTOR 3 CONTROL
E4 | 0.75 | 3LC | + INJECTOR 4
F4 | 0.75 | 3KZ | INJECTOR 4 CONTROL
G4 | 0.75 | 3LA | + INJECTOR 2
H4 | 0.75 | 3KX | INJECTOR 2 CONTROL
M4 | 0.75 | 3HI | FUEL PRESSURE CONTROL SOLENOID VALVE - CONTROL