R13

| CONNECTION
ANY TYPE

#### R13
LEFT REAR/LEFT-HAND REAR DOOR CONNECTION
X84 B84,S84/DG/SPRGAZ/EBASE X84 B84,S84/DG/EQGPL/EBASE

1 | 1.0 | 34A | LEFT HAND REAR LOUDSPEAKER + SIGNAL
2 | 1.0 | 34B | LEFT HAND REAR LOUDSPEAKER - SIGNAL
3 | 0.5 | 20BK | PASSENGER DOORS / REAR DOORS LOCKING MOTOR CONTROL
3 | 1.0 | 20BK | PASSENGER DOORS / REAR DOORS LOCKING MOTOR CONTROL
4 | 0.5 | 20BD | OPEN FRONT/REAR PASSENGER DOORS MOTOR CONTROL
4 | 1.0 | 20BD | OPEN FRONT/REAR PASSENGER DOORS MOTOR CONTROL
5 | 0.35 | MZ | REAR END PANEL ELECTRICAL EARTH
6 | 0.35 | 87A | LEFT HAND REAR 1st POSITION SWITCH - SIGNAL