R369

| CONNECTION
ANY TYPE

#### R369
DASH BOARD / MULTIMEDIA CONNECTION
DG RAD03/NINAV3

1 | 1.4 | MAN | DASHBOARD RIGHT-HAND CROSS MEMBER ELECTRICAL EARTH
3 | 0.35 | 47F | VEHICLE SPEED SIGNAL
3 | 0.35 | 47F | VEHICLE SPEED SIGNAL
6 | 0.5 | LPG | PROTECTED LEFT HAND SIDE LIGHT +
10 | 0.5 | AP43 | PROTECED + AFTER IGNITION FUSE
11 | 0.5 | SP2 | PROTECTED + ACCESSORIES > RADIO
11 | 1.0 | SP2 | PROTECTED + ACCESSORIES > RADIO
12 | 0.35 | 133B | INSTRUMENT PANEL CAN H SIGNAL > COMPUTER
13 | 0.35 | 133C | INSTRUMENT PANEL CAN L SIGNAL > COMPUTER
14 | 0.35 | 107G | HANDS FREE TELEPHONE MICROPHONE +
15 | 0.35 | 107H | HANDS FREE TELEPHONE MICROPHONE -
16 | 0.35 | 34DR | RADIO CANH SIGNAL
17 | 0.35 | 34DS | RADIO CANL SIGNAL
18 | 0.35 | 34GD | COMMUNICATION START/STOP SIGNAL 1
18 | 0.35 | 34GD | COMMUNICATION START/STOP SIGNAL 1
19 | 0.35 | 34AM | WAVE SEPARATOR AERIAL AMPLIFIER +
20 | 2.5 | BCP3 | PROTECTED + BATTERY FEED CIRCUIT BREAKER INTERIOR LIGHT FUSE