240

| FRONT PASSENGER DOOR WIRING
X84

#### 240
PASSENGER ELECTRIC REAR-VIEW MIRROR
B84,S84/DD/CPE

1 | 0.35 | 15RP | PROTECTED HEATED REAR VIEW MIRROR + CONTROL
2 | 0.35 | 40B | PASSENGER REAR VIEW MIRROR UP/DOWN CONTROL
3 | 0.35 | 40E | REAR VIEW MIRROR MOTOR COMMON
4 | 0.35 | 40D | PASSENGER REAR VIEW MIRROR RIGHT>LEFT CONTROL
5 | 0.35 | MAM | DASHBOARD LEFT-HAND CROSS MEMBER ELECTRICAL EARTH
5 | 0.35 | MAM | DASHBOARD LEFT-HAND CROSS MEMBER ELECTRICAL EARTH
7 | 0.35 | 40X | REAR-VIEW MIRROR FOLD OUT CONTROL
9 | 0.35 | 40W | REAR-VIEW MIRROR FOLD IN CONTROL