204

| FRONT PASSENGER DOOR WIRING
X84

#### 204
PASSENGER ELECTRIC WINDOW MOTOR
B84,S84/DD/CPE

1 | 0.5 | 22B | PASSENGER'S ELECTRIC WINDOW DOWN CONTROL
2 | 0.5 | 22A | PASSENGER'S ELECTRIC WINDOW UP CONTROL
3 | 2.0 | MAM | DASHBOARD LEFT-HAND CROSS MEMBER ELECTRICAL EARTH
4 | 1.4 | BP70 | PROTECTED + BATTERY FEED > PASSENGER'S ONE-TOUCH FRONT ELECTRIC WINDOW FUSE
6 | 0.5 | 21K | ANTI-PINCH SUNROOF/ELECTRIC WINDOW SERIAL LINE SIGNAL