R3

| CONNECTION
ANY TYPE

#### R3
DASHBOARD/DRIVER'S DOOR CONNECTION
X84 B84,S84/LVAVEL/DG X84 C84,G84/LVAVEL/DG

10 | 2.0 | A1 | + AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY
11 | 3.0 | MAM | DASHBOARD LEFT-HAND CROSS MEMBER ELECTRICAL EARTH
12 | 0.5 | MAM | DASHBOARD LEFT-HAND CROSS MEMBER ELECTRICAL EARTH
20 | 1.4 | 22C | FRONT ELECTRIC WINDOW CONTROL 1
1 | 1.4 | 22D | FRONT ELECTRIC WINDOW CONTROL 2
2 | 0.5 | 20BH | DRIVER'S DOOR / FUEL FILLER FLAP LOCK MOTOR CONTROL
3 | 0.5 | 20BC | DRIVER'S DOOR / FUEL FILLER FLAP UNLOCKING MOTOR CONTROL
4 | 0.5 | 87H | DRIVER'S 1st POSITION SWITCH - SIGNAL
6 | 1.0 | 34G | LEFT HAND FRONT LOUDSPEAKER + SIGNAL
7 | 1.0 | 34H | LEFT HAND FRONT LOUDSPEAKER - SIGNAL
8 | 0.5 | LPG | PROTECTED LEFT HAND SIDE LIGHT +