R243

| CONNECTION
ANY TYPE

#### R243
RIGHT-HAND REAR DOOR/REAR LEFT-HAND WIRING CONNECTION
X84 B84,S84/DG/SPRGAZ/EBASE X84 B84,S84/DG/EQGPL/EBASE

1 | 1.0 | 34D | RIGHT HAND REAR LOUDSPEAKER + SIGNAL
2 | 1.0 | 34C | RIGHT HAND REAR LOUDSPEAKER - SIGNAL
3 | 0.35 | 87B | RIGHT HAND REAR 1st POSITION SWITCH - SIGNAL
4 | 0.35 | MAQ | REAR RIGHT-HAND END PANEL ELECTRICAL EARTH
5 | 0.5 | 20BD | OPEN FRONT/REAR PASSENGER DOORS MOTOR CONTROL
6 | 0.5 | 20BK | PASSENGER DOORS / REAR DOORS LOCKING MOTOR CONTROL