1337

| ENGINE WIRING
K4M760,K4M761

#### 1337
SWITCHING PROTECTION UNIT
BVA4

1 | 1.0 | BP42 | PROTECTED + BATTERY FEED > AUTOMATIC TRANSMISSION COMPUTER
5 | 1.0 | 38R | AIR CONDITIONING CLUTCH + CONTROL
6 | 0.5 | AP11 | PROTECTED + AFTER IGNITION REVERSING LIGHTS FUSE
8 | 2.0 | 3BS | IGNITION COIL CONTROL
9 | 0.75 | H66P | REVERSING LIGHTS + CONTROL
10 | 2.0 | AP4 | PROTECTED + AFTER IGNITION AUTOMATIC TRANSMISSION FUSE