227

| FRONT END WIRING
X84

#### 227
LEFT-HAND HEADLIGHT
LADECH

2 | 0.5 | HK | DIAGNOSTIC SIGNAL K
3 | 1.0 | CPG | PROTECTED LEFT HAND DIPPED BEAM HEADLIGHT +
4 | 1.0 | MAS | FRONT LEFT-HAND SIDE MEMBER ELECTRONIC EARTH
5 | 1.0 | RPG | LEFT HAND PROTECTED MAIN BEAM HEADLIGHT +
6 | 0.5 | 103A | HEADLIGHT POSITION CONTROL
7 | 0.5 | 47F | VEHICLE SPEED SIGNAL
8 | 0.5 | 64C | LEFT HAND TURN SIGNAL LIGHTS CONTROL
9 | 0.35 | LPG | PROTECTED LEFT HAND SIDE LIGHT +
10 | 1.0 | MAS | FRONT LEFT-HAND SIDE MEMBER ELECTRONIC EARTH