R339

| CONNECTION
ANY TYPE

#### R339
ROOF / SUNROOF
TOELEC/TOELEF -

2 | 0.35 | XXXX | EMPTY CONNECTION
3 | 0.35 | 52G | 1-BIT DIGITAL CONTROL
4 | 0.35 | 52J | 3-BIT DIGITAL CONTROL
5 | 0.35 | 52H | 2-BIT DIGITAL CONTROL
6 | 0.35 | 52D | DIGITAL CONTROL EARTH
7 | 0.35 | 47F | VEHICLE SPEED SIGNAL
8 | 0.35 | 21K | ANTI-PINCH SUNROOF/ELECTRIC WINDOW SERIAL LINE SIGNAL
9 | 2.0 | BP93 | + BATTERY PROTECTED SUNROOF
10 | 2.0 | MAM | DASHBOARD LEFT-HAND CROSS MEMBER ELECTRICAL EARTH