R301

| CONNECTION
ANY TYPE

#### R301
DASHBOARD/COURTESY LIGHT CONNECTION
TN SPRTEL TN PRETEL/EBASE TN PRETEL/EPACK TOELEC/TOELEF

1 | 0.35 | BPT | PROTECTED + BATTERY FEED TIMER
2 | 0.35 | MAM | DASHBOARD LEFT-HAND CROSS MEMBER ELECTRICAL EARTH
3 | 0.35 | 13E | INTERIOR LIGHTS - CONTROL > TIMER
7 | 0.35 | 47F | VEHICLE SPEED SIGNAL
8 | 0.35 | 21K | ANTI-PINCH SUNROOF/ELECTRIC WINDOW SERIAL LINE SIGNAL
9 | 2.0 | BP93 | + BATTERY PROTECTED SUNROOF
10 | 2.0 | MAM | DASHBOARD LEFT-HAND CROSS MEMBER ELECTRICAL EARTH